# This file is an output of a discrete event simulation.
# It contains spanning tree information to be parsed while
# visualizing the spanning tree using the Protocols->STP menu.
# Legend: node name, VID, VLAN/tree name, port/node type, link name.
cy.node_4,0,Common ST,root,none
cy.node_4,0,Common ST,designated_port,cy.ftp_server <-> node_4
cy.node_4,0,Common ST,designated_port,cy.cyuser3 <-> node_4
cy.node_4,0,Common ST,designated_port,cy.cyusers <-> node_4
cy.node_4,0,Common ST,designated_port,cy.cyuser1 <-> node_4
cy.node_4,0,Common ST,designated_port,cy.cyuser2 <-> node_4
cy.node_4,0,Common ST,designated_port,cy.node_4 <-> cyrouter
cy.node_4,0,Common ST,designated_port,cy.video_server <-> node_4
usa.node_4,0,Common ST,root,none
usa.node_4,0,Common ST,designated_port,usa.node_4 <-> usa_router
usa.node_4,0,Common ST,designated_port,usa.usauser3 <-> node_4
usa.node_4,0,Common ST,designated_port,usa.usausers <-> node_4
usa.node_4,0,Common ST,designated_port,usa.usauser1 <-> node_4
usa.node_4,0,Common ST,designated_port,usa.usauser2 <-> node_4
cape.node_4,0,Common ST,root,none
cape.node_4,0,Common ST,designated_port,cape.node_4 <-> cape_router
cape.node_4,0,Common ST,designated_port,cape.capeuser3 <-> node_4
cape.node_4,0,Common ST,designated_port,cape.capeusers <-> node_4
cape.node_4,0,Common ST,designated_port,cape.capeuser1 <-> node_4
cape.node_4,0,Common ST,designated_port,cape.capeuser2 <-> node_4
